Package: realTimeloads
Title: Analyte Flux and Load from Estimates of Concentration and
        Discharge
Version: 1.0.0
Authors@R: 
    person(given = "Daniel",
           family = "Livsey",
           role = c("aut", "cre","cph"),
           email = "livsey.daniel@gmail.com",
           comment = c(ORCID = "0000-0002-2028-6128"))
Description: Flux (mass per unit time) and Load (mass) are computed from timeseries estimates of analyte concentration and discharge. Concentration timeseries are computed from regression between surrogate and user-provided analyte. Uncertainty in calculations is estimated using bootstrap resampling. Code for the processing of acoustic backscatter from horizontally profiling acoustic Doppler current profilers is provided. All methods detailed in Livsey et al (2020) <doi:10.1007/s12237-020-00734-z>, Livsey et al (2023) <doi:10.1029/2022WR033982>, and references therein.
License: GPL (>= 3)
Encoding: UTF-8
LazyData: true
RoxygenNote: 7.2.3
Depends: R (>= 2.10)
Imports: data.table, graphics, imputeTS, mice, signal, stats,
        TideHarmonics, utils
Suggests: knitr, rmarkdown
VignetteBuilder: knitr
NeedsCompilation: no
Packaged: 2023-10-17 00:03:34 UTC; livseyd
Author: Daniel Livsey [aut, cre, cph] (<https://orcid.org/0000-0002-2028-6128>)
Maintainer: Daniel Livsey <livsey.daniel@gmail.com>
Repository: CRAN
Date/Publication: 2023-10-18 14:00:02 UTC
Built: R 4.5.2; ; 2025-11-01 03:50:17 UTC; windows
